For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rear Wiper Arm Nut Finish Cap
2 | Rear Wiper Arm Nut Notice: Refer to Fastener Notice in the Preface section. Tip: Hold the blade tip on the first defroster grid line while torquing the wiper arm nut. Tighten
10 N·m (89 lb in)

3 | Windshield Washer Arm Assembly Tip

• | Position wiper blade assembly above the blackout strip as shown in the illustration.

• | Position the blade element on the first defroster grid line, above the blackout.

• | Secure the nut.

• | Install the rear wiper arm nut finish cap.

• | Operate the windshield wipers and inspect for proper operation.