For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove either the LF or RF wheelhouse liner in order to access the fog lamp assembly. Refer to Front Wheelhouse Liner Replacement.

1 | Forward Lamp Harness Connector
2 | Warning: Refer to Halogen Bulb Warning in the Preface section. Fog Lamp Bulb Tip Rotate the lamp socket a quarter turn counter-clockwise and remove the bulb socket.