For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Primary Hood Latch Bolts (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tip Mark the hood latch location to the support bracket with a grease pencil before removing the bolts. Tighten
10 N·m (89 lb in)

2 | Primary Hood Latch Tip

1. Disconnect the hood latch release cable.
2. Disconnect any electrical connectors if equipped.