For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove door handle bezel. Refer to Door Handle Bezel Replacement .

1 | Rear Side Door Trim Panel Plug
2 | Rear Side Door Trim Panel Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 2.5 N·m (22 lb in)
3 | Rear Side Door Trim Panel Assembly
4 | Rear Side Door Trim Panel Retainer (Qty: 12)