For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the steering column. Refer to Steering Column Replacement.

1 | Metal Collar Rake Pivot
2 | Plastic Bushing (Qty: 2) Tip During installation, use NEW bushings.
3 | Anti-Rotation Bracket Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 5 N·m (44 lb in)
4 | Anti-Rotation Bracket
5 | Steering Angle Sensor

#### Procedure

Disconnect any electrical connectors as needed.