For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .
2. Remove the engine mount strut to bracket bolts (1).
3. Rotate strut (2) vertical then remove engine mount strut to side rail nuts (3).
4. Remove the strut from vehicle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Position the strut (2) to the side rail, then install the strut to side rail nuts (3).

Tighten
Tighten the nuts to 110 N·m (81 lb ft).

2. Install the engine mount strut to bracket bolts (1).

Tighten
Tighten the bolts to 25 N·m (18 lb ft).

3. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .