For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the liftgate center applique panel. Refer to Liftgate Center Applique Replacement.

1 | Rear Window Wiper Motor Bolts (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten Tighten the rear window wiper motor bolts in the sequence as shown to 10 N·m (89 lb in)
2 | Rear Window Wiper Motor Tip Pull the motor forward, disconnect the electrical connector and remove the wiper motor shaft grommet.