For 1990-2009 cars

Important: Do not damage the wiring harness connectors.

1. Disconnect the wiring harness connectors 1-8.
2. Remove the fluid temperature sensor bolt (31).
3. Remove the fluid temperature sensor clamp (49).
4. Remove the fluid temperature sensor (36) and the O-ring (32) from the control valve body assembly.
5. Remove the A/T control wiring harness connector retainer (69).

Important: Do not break the wiring harness connectors or the fluid temperature sensor.

6. Remove the transmission wiring harness assembly (33) from the transmission case assembly through the wiring harness bore.
7. Remove the TCM seal (72) and the automatic transmission wiring connector seal (46) from the connector.