For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Brake Dust Caution in the Preface section.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear tire and wheel. Refer to Tire and Wheel Removal and Installation .
3. Remove the rear brake rotor. Refer to Rear Brake Rotor Replacement .

1 | Park Brake Shoe Hold Down Spring (Qty: 2)

#### Procedure

Compress the spring and rotate ¼ turn to release.

2 | Park Brake Shoe Hold Down Spring Pin (Qty: 2)
3 | Park Brake Shoe Adjuster Spring

#### Procedure

Using the J 38400 , remove the adjuster spring.

#### Tools Required

J 38400 Brake Shoe Spanner and Spring Remover

4 | Park Brake Shoe Adjuster Screw

#### Procedure

Clean the threads and apply high temperature grease to the adjuster screw.

5 | Park Brake Shoe Return Spring

#### Procedure

Using the J 38400 , remove the return spring.

#### Tools Required

J 38400 Brake Shoe Spanner and Spring Remover

6 | Park Brake Shoe (Qty: 2)

#### Procedure

1. Use denatured alcohol to clean brake dust or grease from the park brake shoes and hardware.
2. If reinstalling the park brake shoes, note the location of the park brake shoes for installation.
3. Apply a small amount of high temperature silicone grease to the brake shoe and backing plate contact points.
4. Adjust the park brake. Refer to Park Brake Adjustment .