For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front wheel and tire assemblies. Refer to Tire and Wheel Removal and Installation.

1 | Stabilizer Shaft Insulator Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 50 N·m (37 lb ft).
2 | Stabilizer Shaft Insulator Clamp (Qty: 2)
3 | Stabilizer Shaft Insulator (Qty: 2)