For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to SIR Caution in the Preface section.

#### Preliminary Procedure

Remove the inflatable restraint steering wheel module. Refer to Inflatable Restraint Steering Wheel Module Replacement .

Tip
Right hand steering wheel control switch shown. Left hand similar.

1 | Steering Wheel Trim Cover Bolt (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Steering Wheel Trim Cover (Qty: 2)
3 | Steering Wheel Control Switch Assembly Screw (Qty: 6) Tip DO NOT over tighten the steering wheel control switch screws or damage to the switch(s) or steering wheel covers may occur. Tighten 2 N·m (18 lb in)
4 | Steering Wheel Control Switch Assembly (Qty: 2) Tip Make sure the steering wheel control switch(s) are properly seated to the steering wheel shroud during installation.