For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to SIR Inflator Module Handling and Storage Caution in the Preface section.

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling .
2. Remove center pillar lower molding. Refer to Center Pillar Lower Garnish Molding Replacement .
3. Release seat belt from seat side anchor.

1 | Seat Belt Retractor Pretensioner Adjuster Cover
2 | Seat Belt Retractor Pretensioner Bolt Notice: Refer to Fastener Notice in the Preface section. Tip Apply GM P/N 12345382 (Canadian P/N 10953489), Permatex® 24200 or equivalent on all restraint fasteners prior to installation. Tighten
45 N·m (33 lb ft)

3 | Seat Belt Retractor Pretensioner Adjuster Bolt Tighten 45 N·m (33 lb ft)
4 | Seat Belt Retractor Pretensioner Assembly

#### Procedure

1. Disconnect the electrical connectors.
2. Discharge and dispose of pretensioner assembly using the appropriate procedure. Refer to Pretensioner Handling and Scrapping .