For 1990-2009 cars

### Removal Procedure

1. Remove the radiator outlet hose. Refer to Radiator Outlet Hose Replacement.
2. Remove the water outlet housing bolts (1).
3. Remove the housing.
4. Remove the water outlet housing O-ring seal (2).
5. Remove the water outlet housing seal (3). Discard seal.

### Installation Procedure

1. Install a NEW water outlet housing seal (3).
2. Install a NEW water outlet housing O-ring seal (2).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the water outlet housing bolts (1).

Tighten
Tighten the water outlet housing bolts to 10 N·m (89 lb in).

4. Install the radiator outlet hose. Refer to Radiator Outlet Hose Replacement.