For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the underhood electrical center or junction block. Refer to Underhood Electrical Center or Junction Block Replacement.

1 | Underhood Electrical Center or Junction Block Bracket Bolt Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

Remove the electrical connector inside the block before removing the bracket.

Tighten
20 N·m (15 lb ft)

2 | Underhood Electrical Center or Junction Block Bracket