For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove third row rear seats. Refer to Rear Number 2 Seat Replacement .

1 | Seat Cushion Inner Finish Trim Panel Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb ft)
2 | Seat Cushion Inner Finish Trim Panel
3 | Seat Belt Buckle Bolt Tighten 45 N·m (33 lb ft)
4 | Seat Belt Buckle Assembly