For 1990-2009 cars

### Removal Procedure

1. Position the seat fully forward.
2. Disconnect the shoulder belt from the seat quick disconnect feature by using a flat-bladed tool to press the tab.
3. Remove the front seat adjuster bolts.
4. Move the seat to the full rearward position.
5. Disconnect the seat electrical connectors.
6. Lift the front seat adjuster hooks from the floor pan.
7. Remove the seat from the vehicle.

### Installation Procedure

Important: This step must be performed to assure proper timing of the adjusters.

1. Adjust the seat adjuster tracks to the fully rearward position.
2. Position the seat in the vehicle and engage the front adjuster hooks in the floor pan.
3. Connect the seat electrical connectors.
4. Position the seat in the fully forward position to expose the rear bolt locations.

Notice: Refer to Fastener Notice in the Preface section.

5. Install the seat adjuster-to-floor bolts.

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

6. Install the shoulder belt webbing in the quick disconnect anchor.
7. Inspect the front seat belt for proper operation.