For 1990-2009 cars

System | DTCs Required to Set System Status to YES
--- | ---
If an I/M System Status indicator did NOT update to YES during the Inspection/Maintenance (I/M) System Check , review each indicator and reference this table to determine each DTC associated with the I/M System Status Indicator. Each DTC listed below has specific conditions that must be met for the diagnostic to run. Included within the conditions are additional DTCs, which if set, may inhibit the DTCs listed below from running. Reviewing and operating the vehicle within the Conditions for Running for each DTC listed below will allow the I/M System Status Indicators to transition to YES.
Catalyst | DTC P0420 or P0430
EVAP | DTC P0442 DTC P0446 DTC P0455 DTC P0496
Oxygen Sensor | DTC P0131 or P0151 DTC P0132 or P0152 DTC P0133 or P0153 DTC P0137, P0138, P0140, P0157, P0158, or P0160 DTC P2096 or P2098

DTC P2097 or P2099

DTC P2231 or P2234

DTC P2232 or P2235

DTC P2270 or P2272

DTC P2271 or P2273

Oxygen Sensor Heater | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 DTC P0135, P0141, P0155, or P0161