For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the battery. Refer to Battery Negative Cable Disconnection and Connection.

1 | Fuse Panel
2 | Instrument Panel Wiring Harness Junction Block Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
3 | Instrument Panel Wiring Harness Junction Block Assembly

#### Procedure

Disconnect the electrical connector.