For 1990-2009 cars

## Rear Seat Head Restraint Replacement Outer

Callout | Component Name
--- | ---
1 | Rear Seat Head Restraint

#### Procedure

1. Push the button in and raise the head restraint to the full-up position.
2. Insert a small round tool into the guide hole
3. Pull up to remove the head restraint.

## Rear Seat Head Restraint Replacement Inner

Callout | Component Name
--- | ---
1 | Rear Center Seat Head Restraint

#### Procedure

1. Push the button in and raise the head restraint to the full-up position.
2. Insert a small round tool into the guide hole
3. Pull up to remove the head restraint.