For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to SIR Caution in the Preface section.

#### Preliminary Procedures

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling .
2. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .
3. Remove the front door check link. Refer to Rear Side Door Check Link Replacement .

1 | Rear Side Door Upper Hinge Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

1. Remove the water deflector.
2. Support the door before removing the hinge bolts.
3. Disconnect the electrical connector, if equipped.
4. With the aid of an assistant, remove the door.

Tighten
31 N·m (23 lb ft)

2 | Rear Side Door Lower Hinge Bolt (Qty: 2) Tighten 31 N·m (23 lb ft)
3 | Rear Side Door

#### Procedure

When replacing the door it is necessary to transfer all of the internal components.