For 1990-2009 cars

### Inside Rearview Mirror with the Automatic Day-Night Feature System Components

The inside rearview mirror with the automatic day-night feature system consist of the following component:

Inside rearview mirror

### Power and Ground of the Inside Rearview Mirror

• | With the ignition ON, ignition voltage is supplied to the mirror from the POWER SUNROOF20A fuse in the I/P fuse block.

• | Ground for the mirror is provided by G401.

### Inside Rearview Mirror with the Automatic Day-Night Feature System Operation

The inside rearview mirror uses 2 photocell sensors. One sensor is the headlight sensor, located on the rear side of the mirror. The headlight sensor is used to determine light conditions present at the mirror face. The other sensor is the ambient light sensor, located on the front of the mirror or windshield side. The ambient light sensor is used to determine light conditions present at the mirror. With automatic day-night feature enabled, the mirror uses ambient light sensor to determine the exterior light condition. With a low light condition detected, and a high light condition from behind at the headlight sensor, the inside rearview mirror will automatically darken the face of the mirror.

In the daytime, the mirror is in a normal state because of the high light condition that is indicated by the ambient light sensor. With the gear selector lever in the REVERSE position, backup lamp supply voltage is supplied as an input to the inside rearview mirror. In night time conditions only, the mirror monitors this input to disable the automatic day-night feature which allows the face to gradually change to a normal state. This allows the driver to see objects in the mirror clearly when backing up.