For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Engage the Parking Brake.
2. Place the shifter in the neutral position.
3. Remove the Shifter Knob. Refer to Transmission Control Lever Knob Replacement .

1 | Instrument Panel Lower Brace Bezel Assembly

#### Procedure

1. Use a flat bladed plastic trim tool in order to release the bezel from the I/P.
2. Disconnect the electrical connections.
3. When replacing the lower I/P brace bezel, transfer all necessary components.

2 | Retainer Clips (Qty 4)