For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the right rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement .

1 | Radio Rear Compartment Speaker Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Radio Rear Compartment Speaker Nut (Qty: 2) Tighten 2.5 N·m (22 lb in)
3 | Radio Rear Compartment Speaker

#### Procedure

1. Disconnect the electrical connectors.
2. Transfer the amplifier assembly to the new speaker.