For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove rear floor storage bin. Refer to Rear Storage Compartment Replacement .
2. Remove third row seat. Refer to Rear Number 2 Seat Replacement .
3. Remove liftgate door sill plate. Refer to Liftgate Door Sill Plate Replacement .
4. Remove the rear carpet retainer. Refer to Rear Carpet Retainer Replacement .
5. Remove rear seat #2 seat belt anchor bolt. Refer to Seat Belt Retractor Replacement - No. 2 Rear .

1 | Rear Quarter Lower Trim Plug
2 | Rear Quarter Lower Trim Panel Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 2.5 N·m (22 lb in)
3 | Rear Quarter Lower Trim Panel Clip (Qty: 9)
4 | Rear Quarter Lower Trim Panel Retainer (Qty: 5)
5 | Rear Quarter Lower Trim Panel Assembly Tip Disconnect electrical connector.