For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Number 2 Seat Replacement .
2. Remove the rear seat inner recliner cover. Refer to Rear Seat Back Recliner Cover Replacement .
3. Remove the rear seat back outer finish panel.
4. Remove the seat cushion front finish cover. Refer to Rear Seat Number 2 Cushion Trim Panel Replacement .

1 | Rear Seat No. 2 Cushion Cover Disconnect the seat cushion cover j-channel from the seat cushion frame.
2 | Rear Seat No. 2 Cushion Pad