For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector from the blower motor control module.
2. Remove the blower motor control module screws from the HVAC module.
3. Remove the blower motor control module from the HVAC module.

### Installation Procedure

1. Install the blower motor control module to the HVAC module.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the blower motor control module screws to the HVAC module.

Tighten the screws to 1.5 N·m (13 lb in).

3. Connect the electrical connector to the blower motor control module.