For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear differential assembly from the vehicle. Refer to Differential Replacement.

1 | Rear Differential Vent

#### Procedure

1. Remove any dirt or debris from the vent area.
2. Using an appropriate pair of pliers, remove the vent from the rear differential housing.

Tip

• | The rear differential does not have to be removed from the jack stand to perform this procedure.

• | When installing the vent, use a deep well socket that fits on the flange of the vent and gently tap the vent into place.