For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to Brake Dust Warning in the Preface section. Caution: Support the brake caliper with heavy mechanic wire, or equivalent, whenever it is separated from its mount and the hydraulic flexible brake hose is still connected. Failure to support the caliper in this manner will cause the flexible brake hose to bear the weight of the caliper, which may cause damage to the brake hose and in turn may cause a brake fluid leak.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation.
3. Without disconnecting the brake caliper flexible hose, remove the brake caliper and support with heavy mechanics wire or equivalent. Refer to Front Brake Caliper Replacement.
4. Remove the brake pads.

1 | Brake Caliper Bracket Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. If reusing the brake caliper bracket bolt, the threads of the caliper bracket bolt and the threads of the knuckle mounting holes must be free of threadlocker residue and debris prior to the application of threadlocker to ensure proper adhesion and fastener retention.
2. If reusing the brake caliper bracket bolt, prepare the caliper bracket bolt and the knuckle mounting holes as follows:

2.1. | Thoroughly clean the threadlocker residue from the brake caliper bracket bolt threads with denatured alcohol or equivalent and allow to dry.

2.2. | Thoroughly clean the threadlocker residue from the knuckle mounting holes with denatured alcohol or equivalent and allow to dry.

2.3. | Apply high temperature, high strength threadlocker to 2/3 of the threaded length of the brake caliper bracket bolt. Ensure there are no gaps along the length of the filled area of the caliper bracket bolt.

2.4. | Allow the threadlocker to cure approximately 10 minutes before installing the guide pin bolt.

Tighten
185 N·m (136 lb ft)

2 | Brake Caliper Bracket