For 1990-2009 cars

### Removal Procedure

Important: The evaporative emission (EVAP) canister filter cover must also be replaced when the EVAP filter is replaced to ensure proper operation of the EVAP canister.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the EVAP canister. Refer to Evaporative Emission Canister Replacement.
3. Carefully release the canister filter cover rear retaining tabs.
4. Carefully release the canister filter cover forward retaining tabs and remove the cover from the EVAP canister.
5. Discard the EVAP canister filter cover.
6. Remove the filter from the canister and discard the filter.
7. Clean the inside of the EVAP canister filter housing with a clean shop towel.

### Installation Procedure

1. Install a NEW filter to the canister filter housing.

Important: Ensure that the seal is properly seated in the NEW EVAP filter cover.

2. Install a NEW EVAP filter cover to the EVAP canister.
3. Install the EVAP canister. Refer to Evaporative Emission Canister Replacement.
4. Lower the vehicle.