For 1990-2009 cars

1. Place the drive belt idler pulley and bolt in position through the generator mounting hole and into the engine front cover.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the drive belt idler pulley bolt.

Tighten
Tighten the drive belt idler pulley bolt to 50 N·m (37 lb ft).

3. Tighten the generator bolts.

Tighten
Tighten the generator bolts to 50 N·m (37 lb ft).