For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Number 2 Seat Replacement .
2. Remove the rear seat head restraint. Refer to Rear Seat Number 2 Head Restraint Replacement .
3. Remove the rear seat head restraint guides. Refer to Rear Seat Number 2 Head Restraint Guide Replacement .
4. Remove the rear seat back recliner handle. Refer to Rear Seat Recliner Handle Replacement .

1 | Rear Seat No. 2 Back Cover and Pad Refer to Rear Seat Number 2 Back Cushion Cover and Pad Replacement
2 | Rear Seat No. 2 Cushion Cover and Pad Refer to Rear Seat Number 2 Cushion Cover and Pad Replacement .
3 | Rear Seat No. 2 Back Frame Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
4 | Rear Seat No. 2 Back Pivot Bolt Tighten 2 N·m (18 lb in)
5 | Rear Seat No. 2 Back Frame
6 | Rear Seat Back No. 2 Latch Nut (Qty: 4)
7 | Rear Seat Back No. 2 Latch Assembly
8 | Rear Seat Back No. 2 Inner Pivot