For 1990-2009 cars

### Removal Procedure

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling.
2. Remove the front floor console. Refer to Console Replacement.
3. Disconnect the warning lamp switch electrical connector (2).
4. Remove the warning lamp switch mounting screw (1).
5. Remove the switch from the park brake lever assembly.

### Installation Procedure

1. Align the park brake warning lamp switch locating tab to the locating hole on the park brake lever assembly.
2. Install the switch to the park brake lever.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the park brake warning lamp switch mounting screw (1) and tighten to 4 N·m (35 lb in).
4. Connect the park brake warning lamp switch electrical connector (2).
5. Install the front floor console. Refer to Console Replacement.
6. Enable the SIR system. Refer to SIR Disabling and Enabling.
7. Verify correct park brake warning lamp operation.