For 1990-2009 cars

### Removal Procedure

1. Lower the rear side door window.
2. Remove the rear side door trim panel. Refer to Rear Side Door Trim Panel Replacement .
3. Remove the rear side door window belt inner sealing strip. Refer to Rear Side Door Window Inner Sealing Strip Replacement .
4. Starting at one end, carefully pull the window weatherstrip run channel from the door frame.

### Installation Procedure

1. Align the notch in the window weatherstrip seal to the fixed window post and press the weatherstrip onto the window flange.

1.1. | Press the weatherstrip run channel onto the door flange.

1.2. | Ensure the channel is fully secured into the upper corners of the door frame.

2. Install the rear side door window belt inner sealing strip. Refer to Rear Side Door Window Inner Sealing Strip Replacement .
3. Install the rear side door trim panel. Refer Rear Side Door Trim Panel Replacement .