For 1990-2009 cars

#### Special Tools

• | J 8092 Driver Handle

• | J 33832 Rear Bearing Installer

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Drain the rear differential. Refer to Rear Axle Lubricant Replacement .
3. Remove the muffler assembly. Refer to Muffler Replacement .
4. Remove the left rear wheel drive shaft. Refer to Rear Wheel Drive Shaft Replacement .
5. Using the appropriate tool, remove the axle shaft seal (1).

### Installation Procedure

1. Using the J 8092 and the J 33832 , install the axle shaft seal (1).
2. Install the left rear wheel drive shaft. Refer to Rear Wheel Drive Shaft Replacement .
3. Install the muffler assembly. Refer to Muffler Replacement .
4. Fill the rear differential with fluid. Refer to Rear Axle Lubricant Replacement .
5. Remove the support and lower the vehicle.