For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Replace the passenger presence system as a complete assembly to prevent possible injury to the occupant. All the components in the service kit are assembled and calibrated as a unit. Using only some of the components in the service kit will cause the passenger presence system to operate improperly.

Caution: To avoid personal injury, perform a preload test on the passenger presence system whenever you remove or replace the seat cushion trim. Failure to do so may cause the system to malfunction.

Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. Remove the seat cushion cover and pad. Refer to Front Seat Cushion Cover and Pad Replacement .
3. Re-zero the inflatable restraint passenger presence system whenever the seat cushion or any component of the passenger presence system is removed. Refer to Control Module References .
4. Program the inflatable restraint passenger presence system after replacement. Refer to Control Module References .

1 | Inflatable Restraint Front Passenger Presence System Assembly Tip

• | The passenger presence system is an integral part of the pad on the passenger seat cushion.

• | The sensor, module and seat cushion pad must be replaced as a unit.

• | Note the routing of the wiring harness and connector location for installation.