For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the battery tray. Refer to Battery Tray Replacement.
2. Remove the underhood electrical center/junction block. Refer to Underhood Electrical Center or Junction Block Replacement.
3. Remove the left closeout/insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side.

1 | Hood Latch Release Cable Tip Disconnect the cable from the hood latch release cable handle before attempting to remove the cable.