For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the tire/wheel assembly. Refer to Tire and Wheel Removal and Installation .

1 | Rear Wheelhouse Liner Panel Nut Notice: Refer to Fastener Notice in the Preface section. Tighten 4 N·m (35 lb in)
2 | Rear Wheelhouse Liner Panel Bolt Tighten 10 N·m (89 lb in)
3 | Rear Wheelhouse Liner Panel Plastic Retainer (Qty: 10)
4 | Rear Wheelhouse Liner Panel