For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Install the engine support fixture. Refer to Engine Support Fixture.
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Front Transmission Mount Thru Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 110 N·m (81 lb ft)
2 | Front Transmission Mount Bolt (Qty: 4) Tighten 50 N·m (37 lb ft)
3 | Front Transmission Mount Stud Tighten 50 N·m (37 lb ft)
4 | Front Transmission Mount Tip Remove the mount through the top of the engine compartment.