For 1990-2009 cars

1. Position the shift lever in PARK.
2. Release the shift control cable adjustment lock cover retaining tab (1) on the bottom side.
3. Slide the shift control cable adjustment lock cover (2) forward exposing the adjustment lock.
4. Carefully squeeze the adjustment lock tabs (1) inward to disengage the adjustment lock.
5. Lift the shift control cable adjustment lock (3).
6. The shift control cable (1) and cable end (2) are free to slide to proper adjustment. Ensure the shift lever and transmission are both in the PARK position.
7. Depress the shift control cable adjustment lock (1) to lock the adjustment.
8. Slide the shift control cable adjustment lock cover (1) over the adjustment lock.
9. Inspect the operation of the starting system with the shift lever in each position. The engine should only crank when the lever is in the PARK or NEUTRAL position.