For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the knee bolster assembly. Refer to Knee Bolster Replacement .
2. Remove the instrument panel upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement .
3. Remove the left console trim panel. Refer to Front Floor Console Side Trim Panel Replacement - Left Side .

1 | Lower Instrument Panel Trim Panel Assembly Screw (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tip

1. The left lower trim panel, center lower trim panel, and the cluster trim bezel are removed as an assembly.
2. Disconnect the electrical connections.

Tighten
2 N·m (18 lb in)

2 | Retainer Clip (Qty: 2)
3 | Instrument Panel Center Lower Trim Panel Assembly Screw (Qty: 3) Tighten 2 N·m (18 lb in)
4 | Instrument Panel Center Lower Trim Panel Assembly Tip If replacing the center lower trim panel, transfer all necessary components.