For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the multifunction turn signal switch housing. Refer to Multifunction Turn Signal Switch Housing Replacement .

1 | Ignition Lock Cylinder Case Bolt Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

1. Use a small chisel and hammer to back out the ignition lock cylinder case bolt counterclockwise and remove it.
2. When installing a new ignition lock cylinder case bolt continue to tighten it until the head shears off.

2 | Ignition Lock Cylinder Case Strap
3 | Ignition Lock Cylinder Case

#### Procedure

Disconnect any electrical connectors as needed.

Tip
The ignition lock cylinder must be turned to the run position in order to remove and/or install the ignition lock cylinder case.