For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
3. Remove the front catalytic convertor. Refer to Catalytic Converter Replacement - Left Side .
4. Remove the starter solenoid BAT terminal nut.
5. Disconnect the engine harness electrical connector.
6. Remove the starter bolts and starter.

### Installation Procedure

1. Position the starter motor in the engine block.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the starter bolts and tighten to 50 N·m (37 lb ft) .
3. Connect the engine harness electrical connector to the starter.
4. Install the starter solenoid BAT terminal nut and tighten to 10 N·m (89 lb in) .
5. Install the front catalytic convertor. Refer to Catalytic Converter Replacement - Left Side .
6. Lower the vehicle.
7. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .