For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### DTC Descriptor

DTC B3875 00: Wiper High Speed Relay Circuit

### Diagnostic Fault Information

Circuit | Short to Ground | Open/High Resistance | Short to Voltage | Signal Performance
--- | --- | --- | --- | ---
Windshield Wiper Switch High Signal | 2 | 2 | 2 | --
Windshield Wiper Switch Low Signal | 3 | B3922 00 | 3 | --
Windshield Wiper Motor Park Switch Signal | 4 | 4 | -- | --
Windshield Wiper High Speed Relay Control | 2 | 2 | B3875 00 | --
Windshield Wiper Low Speed Relay Control | B3715 02 | 3 | 3 | --
Windshield Wiper Motor High Speed Control | 2 | 2 | 2 | --
Windshield Wiper Motor Low Speed Control | 3 | 3 | 3 | --
Windshield Wiper Washer Switch Ground | -- | 1 | 1 | --
Windshield Wiper Motor Ground | -- | 1 | 1 | --
Underhood Fuse Block Ground | -- | 1 | 1 | --
1. Wipers inoperative in all speeds 2. High speed wiper malfunction 3. Delay and/or low speed wiper malfunction 4. Wipers do not park

### Circuit/System Description

The body control module (BCM) controls the wiper motor based on input from the windshield wiper washer switch. The BCM monitors the wiper washer switch through three separate signal circuits and a ground circuit. The windshield wiper switch high signal circuit is used to determine high speed wiper operation, the windshield wiper switch low signal is used to determine low speed, intermittent, and mist operation through the use of a resistor ladder, and windshield washer switch signal circuit is used to determine washer operation.

The BCM controls the windshield wiper motor through two output controls, controlling two different PCB relays which control the desired wiper speed, high or low.

### Conditions for Running the DTC

A high speed wiper request is present

### Conditions for Setting the DTC

A short to voltage is detected in the windshield wiper high speed relay control circuit

### Action Taken When the DTC Sets

High speed wiper operation is suspended

### Conditions for Clearing the DTC

• | A current DTC will clear when the condition for setting the fault is no longer seen

• | A history DTC will clear after 50 consecutive ignition cycles without a fault present

### Reference Information

#### Schematic Reference

Wiper/Washer Schematics

#### Connector End View Reference

Wiper/Washer Connector End Views

#### Description and Operation

Wiper/Washer System Description and Operation

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### Scan Tool Reference

• | Scan Tool Output Controls

• | Scan Tool Data List

• | Scan Tool Data Definitions

### Circuit/System Verification

Ignition ON, wiper switch in the HIGH position. Verify the windshield wipers are cycling at the high speed.

### Circuit/System Testing

1. Ignition OFF, disconnect the C2 harness connector at the underhood fuse block.
2. Connect a test lamp between the control circuit terminal 31 and B+.
3. Ignition ON, command the high speed wipers ON and OFF using the wiper switch. The test lamp should turn ON and OFF when changing between the commanded states.

⇒ | If the test lamp is always ON, test the control circuit for a short to ground. If the circuit tests normal, replace the BCM.

⇒ | If the test lamp is always OFF, test the control circuit for a short to voltage or an open/high resistance. If the circuit tests normal, replace the BCM.

4. If all circuits test normal, test or replace the underhood fuse block..

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure

• | Underhood Electrical Center or Junction Block Replacement

• | Control Module References for BCM replacement, setup, and programming