For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement.
2. Remove the rear quarter upper trim panel. Refer to Lock Pillar Upper Garnish Molding Replacement.

1 | Rear Seat Belt Retractor Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tip Apply GM P/N 12345382 (Canadian P/N 10953489), Permatex® 24200 or equivalent on all seat belt fasteners prior to installation. Tighten
45 N·m (33 lb ft)

2 | Rear Seat Belt Retractor Tip Make sure alignment slots are aligned correctly on reinstallation.