For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the left rear trim panel. Refer to Quarter Lower Rear Trim Panel Replacement .
2. Remove the vehicle headliner. Refer to Headlining Trim Panel Replacement .
3. Remove the auxiliary duct from the HVAC module. Refer to Auxiliary Air Distributor Duct Replacement - Upper .
4. Remove the auxiliary air duct upper left side portion. Refer to Auxiliary Air Distributor Duct Replacement - Upper .

1 | Auxiliary Air Distribution Duct Push Pins (Qty: 4)
2 | Auxiliary Air Distribution Duct - Upper Tip Follow mandatory sequence upon installation shown in graphic.