For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear center seat belt bolt. Refer to Seat Belt Replacement - Center Rear .

1 | Rear Seat No. 1 Back Shoulder Belt Opening Bezel Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tip Lift up the seat belt to access the screws. Tighten
2 N·m (18 lb in)

2 | Rear Seat No. 1 Back Release Handle Tip The bezel is integral to the rear center seat belt assembly and must be replaced as an assembly.