For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel cluster bezel. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .

1 | Instrument Panel Cluster Assembly Screw (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Instrument Panel Cluster Assembly

#### Procedure

1. Disconnect the electrical connectors.
2. If replacing the cluster assembly, transfer the cluster trim plate cover. Refer to Instrument Panel Cluster Trim Plate Cover Replacement .