For 1990-2009 cars

1. Loosen the suspension adjustment link-to-frame fastener enough to allow for movement.

Important: The frame of the vehicle is slotted, a cam nut is available for service if required.

2. Rotate the suspension adjustment link cam nut in the direction necessary to correct the toe angle.
3. Snug the suspension adjustment link-to-frame fastener, do not tighten at this time.
4. Reinspect the rear toe specifications and adjust as necessary.

Notice: Refer to Fastener Notice in the Preface section.

5. Hold the nut and tighten the link-to-frame fastener bolt.

Tighten
Tighten the bolt to 164 N·m (121 lb ft).

6. Repeat the procedure for the other rear wheel.