For 1990-2009 cars

#### Tools Required

GE-47716 Vac N Fill Coolant Refill Tool

### Removal Procedure

1. Drain the radiator. Refer to Cooling System Draining and Filling .
2. Unscrew the drain plug from the radiator end tank.
3. Remove and discard the O-ring.

### Installation Procedure

1. Install the new O-ring.
2. Install and tighten the drain plug into the end tank drain hole.
3. Fill the radiator. Refer to Cooling System Draining and Filling .