For 1990-2009 cars

#### Special Tools

GE-47716 Vac N Fill Coolant Refill Tool

### Removal Procedure

1. Drain the engine coolant. Refer to Cooling System Draining and Filling .
2. Remove the surge tank inlet hose clamp from the surge tank.
3. Disconnect the surge tank inlet hose from the surge tank.
4. Remove the surge tank bolts from the surge tank.
5. Lift the surge tank to gain access to the heater outlet hose.
6. Remove the heater outlet hose clamp from the surge tank.
7. Remove the heater outlet hose from the surge tank.
8. Remove the surge tank from the vehicle.

### Installation Procedure

1. Install the heater outlet hose to the surge tank.
2. Install the surge tank to the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the surge tank bolts to the surge tank and tighten to 9 N·m (80 lb in) .
4. Connect the surge tank inlet hose to the surge tank.
5. Install the surge tank inlet hose clamp to the surge tank.
6. Fill the engine coolant. Refer to Cooling System Draining and Filling .